Emulation : In [computing](https://en.wikipedia.org/wiki/Computing), an **emulator** is [hardware](https://en.wikipedia.org/wiki/Computer_hardware) or [software](https://en.wikipedia.org/wiki/Software) that enables one [computer system](https://en.wikipedia.org/wiki/Computer_system) (called the *host*)

CLI: Command Line Interface

NVRAM: non-volatile random-access memory, NVRAM (non-volatile random-access memory) refers to computer memory that can hold data even when power to the memory chips has been turned off. NVRAM is a subset of the larger category of non-volatile memory ([NVM](https://www.techtarget.com/searchstorage/definition/nonvolatile-memory)), which includes storage-class memory based on NAND flash.

SVI: switch virtual interface

IOS: Internetwork operating system

Exhibit: publicly display (a work of art or item of interest)

DHCP: Dynamic Host Configuration Protocol

DSL: digital subscriber line

The [Session. Contents](https://docs.microsoft.com/en-us/previous-versions/iis/6.0-sdk/ms525093(v=vs.90)) collection contains all of the items that have been established for a session without using the <OBJECT> tag.